Press information

To download a 300dpi print quality image, go to [parkfield.co.uk/verotec\_us/km6-1-print.jpg](http://www.parkfield.co.uk/verotec_us/km6-1-print.jpg)

To download a Word file of the text, go to [parkfield.co.uk/verotec\_us/km6-1.docx](http://www.parkfield.co.uk/verotec_us/km6-1.docx)

To view all Verotec press information, go to [parkfield.co.uk/verotec\_us/](http://www.parkfield.co.uk/verotec_us/)

**The KM6 family is the ideal card cage for any application**

**Released June 21, 2018**

Verotec’s [KM6 card cage family](http://www.verotec.co.uk/subracks-c-1.html), which conforms to DIN41494 and IEC60297, is arguably the most comprehensive and versatile system available. Originally developed by Vero Electronics, it has continually evolved over time to reflect the changing requirements of the electronics industry. The flagship KM6-II was first introduced 30 years ago; its design, unchanged to this day, has stood the test of time: more than one million units have been supplied to many different sectors. The much newer heavy duty KM6 -HD units meet the requirements of MIL-STD-167, offering an unrivalled combination of strength, versatility and configurability.

KM6-II is available as standard in 3U, 4U, 6U and 9U heights, widths of 24, 42, 60 and 84HP and depths of 160, 240, 300, 360 and 420mm. The range gives an extensive choice of tiebar recess and board depth. Two screw fixings of the tiebars into the side plates gives high structural strength and rigidity, enabling the heaviest boards and modules to be housed with complete confidence.

For use in railway, military and other high shock and vibration environments, the heavy duty  
KM6–HD range, available in heights of 3U, 6U and 9U and depths up to 400mm. It features 3mm thick side panels, deep tiebar extrusions and screw-down card guide mounts to give outstanding protection from shock and vibration. With integral EMC gasketing, a conductive finish throughout, an integral rear plug-up area and guides that provide PCB grounding, an ESD spring position and integral coding, it conforms to the requirements of IEEE1101.10 and 1101.11 for VMEbus, VXI, VME64x, VPX, cPCI, PXI and other open architecture bus-based systems.

A wide choice of EMC kits, anodized or Alochrome conductive finishes, standard plug-in modules and front panels, divider kits, ventilated and plain top and base covers, front and rear panels and thermal management products are available. The majority of accessory products are compatible with both platforms; both variants have their own dedicated range.

\*\*\* Ends: body copy 316 words \*\*\*

**Notes to editors.**

For further information:

Marc Harvey

Verotec Inc  
150 Zachary Road, suite 6

Manchester, NH 03109  
Ph 603.821.9921

Fax 603.821.9923  
[sales@verotec.us](mailto:sales@verotec.us)

[www.verotec.us](http://www.verotec.us)

Agency contact:

Nigel May

Parkfield Communications Limited

Parkfield House

Damerham

SP6 3HQ

tel: + 44 (0)1725 518321

fax: + 44 (0)1725 518378

[nigel.may@parkfield.co.uk](mailto:nigel.may@parkfield.co.uk)

[www.parkfield.co.uk](http://www.parkfield.co.uk)