

Press information

Released 09 June, 2021

To download a 300dpi print quality image, go to [parkfield.co.uk/hammond-usa/1551v-snap-print.jpg](https://www.parkfield.co.uk/hammond-usa/1551v-snap-print.jpg)

To download a Word file of the text, go to [parkfield.co.uk/hammond-usa/1551v-snap.docx](https://www.parkfield.co.uk/hammond-usa/1551v-snap.docx)

To view all Hammond Manufacturing press information, go to [parkfield.co.uk/hammond-usa/](https://www.parkfield.co.uk/hammond-usa/)

**Hammond introduces yet more versions of its 1551 miniature plastic enclosure family**

The 1551 miniature plastic enclosure family from Hammond Manufacturing consists of 49 different sizes; in this latest extension to the range a further 10 variants have been introduced. In addition to the available size and configuration options, a choice of colors, flanged lids, keyring and USB C versions are also available. The [1551V](https://www.hammfg.com/electronics/small-case/plastic/1551v) ventilated sensor enclosure versions have now been extended with the addition of 1.77-, 2.13- and 3.15-inch (45, 60 and 80mm) diameter round versions, available with plain or vented covers. Also added to the 1551V range are unventilated cover versions of the 3.15 x 3.15, 2.36 x 2.36, 1.57 x 1.57 and 3.15 x 1.57 inch (80 x 80, 60 x 60, 40 x 40mm and 80 x 40mm) square and rectangular enclosures.

A key feature of the 1551V design is the snap-fit closure, which allows repeated opening and closing without tools and also maximizes the internal space for PCBs by eliminating screw fixings to secure the cover to the base. The internal real estate available for PCB mounting is 2.89 x 2.89, 2.13 x 2.13, 1.34 x 1.34 and 2.89 x 1.34 inch (74 x 74, 54 x 54, 34 x 34 and 74 x 34mm) in the rectangular units and 1.54, 2.13 and 2.89 inch (39, 54 and 73.50mm) in the circular ones. All options are available in black, grey and white UL94-HB ABS as standard. All bases feature 0.16 inch (4mm) high PCB stand-offs, wall mounting slots and a 15mm cable knock out.

All sizes are 0.79 inch (20mm) high, which gives enough space for board-mounted RJ45, USB and other standard communication interfaces.

\*\*\* Ends: body copy 268 words \*\*\*

**Notes to Editors.**

For further information contact:

Tom Ballou

Hammond Manufacturing Co. Inc.

475 Cayuga Rd.

Cheektowaga

NY 14225-1309
Tel: (716) 630-7030

Fax: (716) 630-7042

tballou@hammfg.com

[www.hammondmfg.com](http://www.hammondmfg.com)

Agency contact:

Nigel May

Parkfield Communications Limited

Parkfield House

Damerham

Hants

SP6 3HQ

United Kingdom

tel: + 44 1725 518321

nigel.may@parkfield.co.uk

[www.parkfield.co.uk](http://www.parkfield.co.uk)

Hammond is one of the world’s leading manufacturers of small plastic, die-cast and metal enclosures for use in the electronics, industrial and electrical industries.