

Press information

Released May 24, 2023

To download a 300dpi print quality image, go to [parkfield.co.uk/hammond-usa/1556-print.jpg](https://www.parkfield.co.uk/hammond-usa/1556-print.jpg)

To download a Word file of the text, go to [parkfield.co.uk/hammond-usa/1556.docx](https://www.parkfield.co.uk/hammond-usa/1556.docx)

To view all Hammond Manufacturing press information, go to [parkfield.co.uk/hammond-usa/](https://www.parkfield.co.uk/hammond-usa/)

**Hammond announces new flame-retardant ABS 1556 family**

The new 14-strong flame-retardant [ABS IP54 1556 family](https://www.hammfg.com/1556), rated UL94-V0, is inspired by our recently launched IP68 polycarbonate 1557 series. It follows the same modern rounded corners and top face styling and introduces rectangular versions to complement the square format versions derived from the 1557 series. IP54 sealed for general purpose indoor use, the ABS material gives a lower price point than the polycarbonate used in the 1557, which is designed for installation outdoors and in aggressive environments. Self-tapping screws secure the lid to the base, making it ideal for applications where repeated opening and closing is not required. It is feature-rich and offer multiple option for configuration and customization. There are multiple PCB mounting standoffs in both the lid and the base.

There are four square plan sizes from 3.15” x 3.15” to 7.87” x 7.87” (80mm x 80mm to 200mm x 200mm) in the range and three rectangular ones from 4.72” x 3.15” to 7.87” x 6.30” (120mm x 80mm to 200mm x 160mm). All sizes are available in two heights, 1.77”, 45mm, and 2.36”, 60mm, for the smallest size and 1.77”, 45mm, and 2.76”, 70mm, for the larger ones in the family. All sizes are available in black, RAL 7035 grey and white. The modern soft rounded styling makes the 1556 an ideal desktop enclosure when fitted with the supplied feet, or it can be wall-mounted with either four visible mounts or two hidden mounts, which are available as optional accessories. Also available as an option for all sizes are 2mm thick aluminum internal panels.

\*\*\* Ends: body copy 240 words \*\*\*

**Notes to Editors.**

For further information contact:

Tom Ballou

Hammond Manufacturing Co. Inc.

475 Cayuga Rd.

Cheektowaga

NY 14225-1309
Tel: (716) 630-7030

Fax: (716) 630-7042

tballou@hammfg.com

[www.hammondmfg.com](http://www.hammondmfg.com)

Agency contact:

Nigel May

Parkfield Communications Limited

Parkfield House

Damerham

Hants

SP6 3HQ

United Kingdom

tel: + 44 1725 518321

nigel.may@parkfield.co.uk

[www.parkfield.co.uk](http://www.parkfield.co.uk)

Hammond is one of the world’s leading manufacturers of small plastic, die-cast and metal enclosures for use in the electronics, industrial and electrical industries.