

Press information

To download a 300dpi print quality image, go to [parkfield.co.uk/hammond-usa/1557-print.jpg](http://www.parkfield.co.uk/hammond-usa/1557-print.jpg)

To download a Word file of the text, go to [parkfield.co.uk/hammond-usa/1557.docx](http://www.parkfield.co.uk/hammond-usa/1557.docx)

To view all Hammond Manufacturing press information, go to [parkfield.co.uk/hammond-usa/](http://www.parkfield.co.uk/hammond-usa/)

**Hammond introduces the stylish new 1557 IP68 wall mount/desktop plastic enclosure family**

Hammond Manufacturing has announced its new [1557 family](https://www.hammfg.com/electronics/small-case/plastic/1557). Initially available in four plan sizes, each in two heights, it is available in polycarbonate, sealed to IP68, and ABS, designed to meet IP66. The sizes are 3.15 x 3.15 x 1.77 and 2.36 inches (80 x 80 x 45 and 60mm) and 4.72 x 4.72, 6.30 x 6.30, 7.87 x 7.87 inches (120 x 120, 160 x 160 and 200 x 200mm) in heights of 1.77 and 2.76 inches (45 and 70mm). All versions are available in black and RAL 7035 grey.

Rounded corners and top face give a modern smooth style, and environmental sealing allows the enclosures to protect the housed equipment against dust and water entry in dirty and damp environments. The 1557 can be used as a free-standing enclosure when fitted with the supplied feet, or it can be wall-mounted with either four visible fixings or two hidden ones. A PDF showing the alternative wall mountings can be [downloaded here](https://www.hammfg.com/files/products/1557/wall-mount-foot-installipt.pdf).

PCB standoffs are provided in both the lid and base. The enclosure is assembled with corrosion-resistant M4 stainless-steel machine screws, which are threaded into integral stainless-steel bushings for repetitive assembly and disassembly. The IP68 polycarbonate versions are UV stabilized for outdoor use with a UL94-5VA rating, the IP66 ABS versions have a flammability rating of UL94-HB for indoor use.

\*\*\*Ends: body copy 199 words \*\*\*

**Notes to Editors.**

**Released November 18, 2019**

For further information contact:

Ray Shatzel

Hammond Manufacturing Co. Inc.

475 Cayuga Rd.

Cheektowaga

NY 14225-1309   
Tel: (716) 630-7030

Fax: (716) 630-7042

[rshatzel@hammfg.com](mailto:rshatzel@hammfg.com)

[www.hammondmfg.com](http://www.hammondmfg.com/)

Agency contact:

Nigel May

Parkfield Communications Limited

Parkfield House

Damerham

Hants

SP6 3HQ

United Kingdom

tel: + 44 1725 518321

fax: + 44 1725 518378

[nigel.may@parkfield.co.uk](mailto:nigel.may@parkfield.co.uk)

[www.parkfield.co.uk](http://www.parkfield.co.uk/)

Hammond is one of the world’s leading manufacturers of small plastic, die-cast and metal enclosures for use in the electronics, electrical and allied industries.