**Press information**

To download a 300dpi print quality image, go to [parkfield.co.uk/bvm/medical-panelpc-print.jpg](http://www.parkfield.co.uk/bvm/medical-panelpc-print.jpg)

To download a Word file of the text, go to [parkfield.co.uk/bvm/medical-panelpc.docx](http://www.parkfield.co.uk/bvm/medical-panelpc.docx)

To view all BVM press information, go to [parkfield.co.uk/bvm/](http://www.parkfield.co.uk/bvm/)

**Lights, camera, action! BVM makes it happen**

While certainly not as glamorous as a film set, but with arguably greater benefits, BVM is supplying medical Panel PC-based systems to a world leader in the storage and transportation of endoscopes. One of their latest developments is a new climate-controlled mobile cart in which endoscopes can be stored for up to 100 days in a surgically sterile aseptic environment, free from contamination caused by harmful bacteria, viruses, or other micro-organisms. The storage unit is controlled and managed by a BVM touchscreen Panel PC optimised to their requirements.

The customer had originally been creating his own hybrid system by combining a commercial TFT monitor with a semi-industrial PC. This was a time-consuming exercise, and when the embedded PC became obsolete, BVM were approached to provide a replacement bespoke system incorporating discreet power and comms cable management and custom i/o in an aesthetically branded single unit. The ultimate design is based on a N3160 Atom Braswell processor on a Mini-ITX motherboard, integrated into a slim-line chassis with a 15-inch 5 wire resistive touchscreen. A customised Windows 10 O/S is optimised to provide graceful shut down in the event of unexpected power loss. The unit offers stable and robust running and future-proofing against potential component obsolescence.

Outsourcing the design and manufacture has allowed the client to allocate engineering resource to develop new software features that enable the sterile cart storage system to be suitable for use anywhere in the world, improving medical investigation procedures.

\*\*\* Ends: body copy 243 words \*\*\*

**Notes to Editors.**

**Released 01 July 2019**

Technical and sales contact for publication:

David Harding

BVM Limited

Lakeside House

Waltham Business Park

Brickyard Road

Swanmore

SO32 2SA

t: + 44 (0)1489 780144

f: + 44 (0)1489 783589

sales@bvmltd.co.uk

[bvm.co.uk/](https://www.bvm.co.uk/)

Editorial contact:

Rod Clarke

t: + 44 (0)1489 780144

rod\_c@bvmltd.co.uk

Agency contact:

Nigel May

Parkfield Communications Ltd

Parkfield House

Damerham

SP6 3HQ

t: + 44 (0)1725 518321

f: + 44 (0)1725 518378

nigel.may@parkfield.co.uk

[parkfield.co.uk](http://www.parkfield.co.uk)